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	Line Break Permit



	Project Name

-
	Project No./Contract No.

     

	Project Location

     
	Requestor Name

     
	Date

     

	Description of Work

     

	Special Instructions

     

	Personal Protective Equipment (PPE) Required
	Check
	
	Other Protective Measures
	Check

	
	Yes
	No
	
	
	Yes
	No

	Air Pack – Approved
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	Barricade - ________ Radius (above/ below)
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Boots – Rubber Boots
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	Blanks to be Installed
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Coveralls  -Tyvek
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	Block Valve Shut
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Film Badge
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	Blower
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Gloves – Long Gloves
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	Fire Extinguisher
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Gloves – Leather Gloves
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	Grating, Floor Opening Covered
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Gloves – Rubber Gloves
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	Lockout Plan Required
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Goggles
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	Piping Support Installed/Needed
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Hood – Acid Hood
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	Planning (Line Break Planning Items Page 2 completed and distributed to all personnel0 involved)
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Respirator – Full-Face Respirator
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	
	
	

	Respirator – Half-Face Respirator
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	Pump Locked Out
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Shield – Face Shield
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	Spark Proof Tiles
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Shield – Special Shielding
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	Standby Person
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Suit – Acid Suit
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	System Less Than 212 °F (100 °C).
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Suit – Hot Suit
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	System Vented
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Suit - Rain
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	Valve Locked Out
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Other:
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	Water Hose
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Other:
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	Other:
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Other:
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	Other:
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Other
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	Other:
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Other:
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	Other:
	 FORMCHECKBOX 

	 FORMCHECKBOX 



	Planning Items for Line Breaks

	1.
	Depressurizing, Cleaning, and Venting Check
	     

	2.
	Nearest Safety Shower Location (if greater than 50 feet [15.2 meters], water hose must be provided)
	     

	3.
	Nearest Eyewash Location
	     

	4.
	Cold Pak Location
	     

	5.
	Scott Air Pak Location
	     

	6.
	Fire Extinguisher Location
	     

	7.
	Fire Alarm Location
	     

	8.
	Stretcher Location
	     

	9.
	Planned Escape Route
	     

	Relaxing PPE Requirements

	Date

     
	Time

     

	PPE reduced to items shown below:

	
	     
	
	     

	
	     
	
	     

	
	     
	
	     

	
	     
	
	     

	
	     
	
	     

	
	     
	
	     

	Approval 

	Name
	Signature
	Date

	Client Representative
	
	

	 Supervisor
	
	

	Person Making Break
	
	

	Person Making Break
	
	

	Line Break Permit Issuer
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